*Intelligent Acoustic Solutions*

TONEWOOD 500

The Oelex ToneWood Slat Wall by Oeler Industries, Inc. is a traditional linear wall and ceiling product that combines

the warmth of wood with excellent acoustical values. We utilize a Class A fire rated no added formaldehyde MDF core covered with your choice of veneer to maximize your finish offerings and to offer straighter lines than solid wood options.

## SIZES & FINISHES

Oelex ToneWood Slat Wall ships in 1’ wide by 8’ long panels with arrangements featuring two to eight blades per panel. The standard finish is a natural clear lacquer. For a more personalized look, choose from 24 standard and 40 custom veneers available, sure to fit any design.

## LEED INFO:

* Credits for MR 4.1, MR 4.2, MR 7, EQ 4.4
* No added Formaldehyde
* FSC certified and offers a chain-of-custody proof of origin

# FEATURES:




## SPEC DATA SHEET # ToneWood-500

4700 Clairton Blvd., Pittsburgh, PA 15236

Tel: (412) 884-3000 • Fax: (412) 884-3300

[www.oeler.com](http://www.oeler.com/) • [sales@oeler.com](mailto:sales@oeler.com)

* + Class A fire rated, CARB2



* + Dowel or backer type assembly based on application
  + Typical blade widths of 5/8", 3/4", 1" or 1-1/4"
  + Typical blade heights of 1-3/4", 2-1/8", 2-1/2" or 3-1/8"
  + Custom sizes available



*Intelligent Acoustic Solutions*

## SPEC DATA SHEET #TONEWOOD-500

**ACOUSTICS:**

As with all Oelex products, acoustical performance is at the fore- front during the design phase of the products. Different acoustical mate- rials can be used both above and behind the grilles to garner acoustical results:

## INSTALLATION:

* Oelex acoustic textile can easily and affordably be added to the back of the grilles
* Oelex black theater board can be incorporated into the design to enhance the acoustical performance

## OPTIONS:

* Typical Grille sections are 12” wide by 8’ long
* Arrangements of 4, 6 or 8 blades per 12” section are standard
* Blades are typically 1 ½’, 2”, 2 ½” or 3” thick

## FINISHES:

* 24 Standard & 40 custom veneers available
* Clear satin lacquer is the standard finish





4700 Clairton Blvd., Pittsburgh, PA 15236

Tel: (412) 884-3000 • Fax: (412) 884-3300

[www.oeler.com](http://www.oeler.com/) • [sales@oeler.com](mailto:sales@oeler.com)

*Intelligent Acoustic Solutions*

Convertible for walls or ceiling arrangements, our proprietary attachment clip provides a solid mounting option along with the ability to access equipment above or behind the grilles. Standard installation will have our attachment clip suspended from a heavy duty 15/16” T-Grid. Installation is simple and the attachment clips works with both the backer and dowel designs.

* + Recessed Wood backer: The black hardwood recessed backer holds the blades securely while disappearing into the background above.
  + Dowel Design: The dowels are often used in open plenum designs where the dowel itself becomes a design element. There are two dowel options. A hardwood (fixed) or a PVC (flexible) option.

## WARRANTY:

All WoodTrends products come standard with a full one-year warranty for manufacturing defects and dimensional stability.